IMPORT
    SELECT_SLOT                      LCARD_AD.SELECT_SLOT,
    PLATA_TEST                       LCARD_AD.PLATA_TEST,
    SET_BOARD_TYPE                   LCARD_AD.SET_BOARD_TYPE,
    GET_BOARD_TYPE                   LCARD_AD.GET_BOARD_TYPE,
    SET_BASE_ADDRESS                 LCARD_AD.SET_BASE_ADDRESS,
    ENABLE_INT                       LCARD_AD.ENABLE_INT,
    CREATE_CHANNEL                   LCARD_AD.CREATE_CHANNEL,
    MEMORY_STATE                     LCARD_AD.MEMORY_STATE,
    MEMORY_PM_STATE                  LCARD_AD.MEMORY_PM_STATE,
    SET_INTER_DELAY                  LCARD_AD.SET_INTER_DELAY,
    SET_ADSP_SPEED                   LCARD_AD.SET_ADSP_SPEED,
    SET_WAIT_STATE                   LCARD_AD.SET_WAIT_STATE,
    SET_TIMER_SCALE                  LCARD_AD.SET_TIMER_SCALE,
    TIMER_L154_L164                  LCARD_AD.TIMER_L154_L164,
    WAIT_TICK_L154_L164              LCARD_AD.WAIT_TICK_L154_L164,
    GET_TIMER_L154_L164              LCARD_AD.GET_TIMER_L154_L164,
    CALIBRATION                      LCARD_AD.CALIBRATION,
    INIT_COMPARATOR                  LCARD_AD.INIT_COMPARATOR,
    LOW_POWER                        LCARD_AD.LOW_POWER,
    GET_SLOT_CODE                    LCARD_AD.GET_SLOT_CODE,
    RESET_ALL                        LCARD_AD.RESET_ALL,
    MAKE_CHANNEL                     LCARD_AD.MAKE_CHANNEL,
    PROGRAM_FILTER                   LCARD_AD.PROGRAM_FILTER,
    PROGRAM_LM_201                   LCARD_AD.PROGRAM_LM_201,
    PROGRAM_LM_102                   LCARD_AD.PROGRAM_LM_102,
    PROGRAM_LM_501                   LCARD_AD.PROGRAM_LM_501,
    PROGRAM_LM_DAC                   LCARD_AD.PROGRAM_LM_DAC,
    GET_LM_401                       LCARD_AD.GET_LM_401,
    LM_404                           LCARD_AD.LM_404,
    PROGRAM_LM_TTLOUT                LCARD_AD.PROGRAM_LM_TTLOUT,
    SETCHANNEL                       LCARD_AD.SETCHANNEL,
    SAMPLE                           LCARD_AD.SAMPLE,
    ADCHAN                           LCARD_AD.ADCHAN,
    KADR                             LCARD_AD.KADR,
    STREAM                           LCARD_AD.STREAM,
    SOFT                             LCARD_AD.SOFT,
    SOFT_HUGE                        LCARD_AD.SOFT_HUGE,
    DMAONE                           LCARD_AD.DMAONE,
    DMAALL                           LCARD_AD.DMAALL,
    DMA_ALL_DA                       LCARD_AD.DMA_ALL_DA,
    OUTDA                            LCARD_AD.OUTDA,
    SET_DA_NUMBER                    LCARD_AD.SET_DA_NUMBER,
    STREAM_OUTDA                     LCARD_AD.STREAM_OUTDA,
    DASTREAM                         LCARD_AD.DASTREAM,
    DASTREAM_HUGE                    LCARD_AD.DASTREAM_HUGE,
    DADMASTREAM                      LCARD_AD.DADMASTREAM,
    OUTBYTE                          LCARD_AD.OUTBYTE,
    INPBYTE                          LCARD_AD.INPBYTE,
    DSP_INPBYTE                      LCARD_AD.DSP_INPBYTE,
    DSP_OUTBYTE                      LCARD_AD.DSP_OUTBYTE,
    INTR_SETUP                       LCARD_AD.INTR_SETUP,
    STOP_INTR                        LCARD_AD.STOP_INTR,
    RESET_IRQ                        LCARD_AD.RESET_IRQ,
    INIT_SIMPLE_INTR                 LCARD_AD.INIT_SIMPLE_INTR,
    STREAM_INTR                      LCARD_AD.STREAM_INTR,
    SOFT_INTR                        LCARD_AD.SOFT_INTR,
    READ_DATA                        LCARD_AD.READ_DATA,
    DATA_READY                       LCARD_AD.DATA_READY,
    SYNCHRO_MODE                     LCARD_AD.SYNCHRO_MODE,
    SOFT_MEMORY_START                LCARD_AD.SOFT_MEMORY_START,
    TEST_FOR_INPUT_END               LCARD_AD.TEST_FOR_INPUT_END,
    GET_INPUT_DATA                   LCARD_AD.GET_INPUT_DATA,
    SOFT_MEMORY_RESTART              LCARD_AD.SOFT_MEMORY_RESTART,
    DMA_OFF                          LCARD_AD.DMA_OFF,
    DMA_TEST                         LCARD_AD.DMA_TEST,
    DMA_COUNTER_IN                   LCARD_AD.DMA_COUNTER_IN,
    DMA_COUNTER_OUT                  LCARD_AD.DMA_COUNTER_OUT,
    GET_BUFFER                       LCARD_AD.GET_BUFFER,
    GET_BUFFER_HALF                  LCARD_AD.GET_BUFFER_HALF,
    PUT_BUFFER                       LCARD_AD.PUT_BUFFER,
    PUT_BUFFER_HALF                  LCARD_AD.PUT_BUFFER_HALF,
    CONFIG_FIFO                      LCARD_AD.CONFIG_FIFO,
    CONFIG_2FIFO_TYPE                LCARD_AD.CONFIG_2FIFO_TYPE,
    READ_FIFO                        LCARD_AD.READ_FIFO,
    STREAM_FIFO2_BEGIN               LCARD_AD.STREAM_FIFO2_BEGIN,
    GET_DIGITS_1056                  LCARD_AD.GET_DIGITS_1056,
    OUT_DIGITS_1056                  LCARD_AD.OUT_DIGITS_1056,
    STREAM_1056                      LCARD_AD.STREAM_1056,
    STREAM_DMA_1056                  LCARD_AD.STREAM_DMA_1056,
    OUT_STREAM_1056                  LCARD_AD.OUT_STREAM_1056,
    OUT_STREAM_DMA_1056              LCARD_AD.OUT_STREAM_DMA_1056,
    INIT_INTR_1056                   LCARD_AD.INIT_INTR_1056,
    SET_SYNCHRO_MODE_1056            LCARD_AD.SET_SYNCHRO_MODE_1056,
    ZERO_MODE_1208                   LCARD_AD.ZERO_MODE_1208,
    OUTDA_1208                       LCARD_AD.OUTDA_1208,
    KADR_1208                        LCARD_AD.KADR_1208,
    SOFT_1208                        LCARD_AD.SOFT_1208,
    SOFT_FON_1208                    LCARD_AD.SOFT_FON_1208,
    DMASOFT_1208                     LCARD_AD.DMASOFT_1208,
    SOFT_INTR_1208                   LCARD_AD.SOFT_INTR_1208,
    GET_DATA                         LCARD_AD.GET_DATA,
    PUT_DATA                         LCARD_AD.PUT_DATA,
    READ_INT_MEMORY                  LCARD_AD.READ_INT_MEMORY,
    WRITE_INT_MEMORY                 LCARD_AD.WRITE_INT_MEMORY,
    LOADBIOS                         LCARD_AD.LOADBIOS,
    POWER_AND_PRINTER_E330           LCARD_AD.POWER_AND_PRINTER_E330,
    SET_EPP_MODE_E330                LCARD_AD.SET_EPP_MODE_E330,
    SET_FIFO_PARAMETERS_E330         LCARD_AD.SET_FIFO_PARAMETERS_E330,
    SET_SOFT_PARM_E330               LCARD_AD.SET_SOFT_PARM_E330,
    SET_TIME_PARAMETERS_E330         LCARD_AD.SET_TIME_PARAMETERS_E330,
    TIMER_INPUT_START_E330           LCARD_AD.TIMER_INPUT_START_E330,
    STOP_FUNC_E330                   LCARD_AD.STOP_FUNC_E330,
    TIMER_INPUT_E330                 LCARD_AD.TIMER_INPUT_E330,
    SOFT_MEMORY_PREPARE_E330         LCARD_AD.SOFT_MEMORY_PREPARE_E330,
    SOFT_MEMORY_START_E330           LCARD_AD.SOFT_MEMORY_START_E330,
    TIMER_INPUT_IRQ_START_E330       LCARD_AD.TIMER_INPUT_IRQ_START_E330,
    IRQ_SLOW_START_E330              LCARD_AD.IRQ_SLOW_START_E330,
    SET_TEST_SPEED_MODE_E330         LCARD_AD.SET_TEST_SPEED_MODE_E330,
    WRITE_BY_ADDRESS_E330            LCARD_AD.WRITE_BY_ADDRESS_E330,
    READ_BY_ADDRESS_E330             LCARD_AD.READ_BY_ADDRESS_E330,
    BOARD_SPECIFIC_INIT              LCARD_AD.BOARD_SPECIFIC_INIT,
    SELECT_BOARD                     LCARD_AD.SELECT_BOARD,
    SETBASEADDRESS                   LCARD_AD.SETBASEADDRESS,
    EXEC_ADSP_COMMAND                LCARD_AD.EXEC_ADSP_COMMAND,
    GET_STATUS                       LCARD_AD.GET_STATUS,
    ALLOCATEBUFFER                   LCARD_AD.ALLOCATEBUFFER,
    CONFIG_TX_CHANNEL_LCI01          LCARD_AD.CONFIG_TX_CHANNEL_LCI01,
    FREEBUFFER                       LCARD_AD.FREEBUFFER,
    GET_HALF_FIFO                    LCARD_AD.GET_HALF_FIFO,
    GET_INPUT_POINTS                 LCARD_AD.GET_INPUT_POINTS,
    QADCHAN                          LCARD_AD.QADCHAN,
    LOADBIOSFROMARRAY_L1211          LCARD_AD.LOADBIOSFROMARRAY_L1211,
    INIT_CORRECTION_LC302            LCARD_AD.INIT_CORRECTION_LC302,
    QSOFT                            LCARD_AD.QSOFT,
    RESERVED2                        LCARD_AD.RESERVED2,
    READ_CALIBR_CC                   LCARD_AD.READ_CALIBR_CC,
    CONFIG_RX_CHANNEL_LCI01          LCARD_AD.CONFIG_RX_CHANNEL_LCI01,
    SELECT_DEVICE                    LCARD_AD.SELECT_DEVICE,
    SET_AD_MODE                      LCARD_AD.SET_AD_MODE,
    CONFIGURE_FAST_READ_CC           LCARD_AD.CONFIGURE_FAST_READ_CC,
    SET_CHANNELS                     LCARD_AD.SET_CHANNELS,
    INITIALIZE_CORRECTION_PC         LCARD_AD.INITIALIZE_CORRECTION_PC,
    SET_DAC_BUFER_E330               LCARD_AD.SET_DAC_BUFER_E330,
    SET_TIME                         LCARD_AD.SET_TIME,
    SET_FAST_PARAMS_CC               LCARD_AD.SET_FAST_PARAMS_CC,
    START_LOOP_DAC_E330              LCARD_AD.START_LOOP_DAC_E330,
    STOP_INPUT                       LCARD_AD.STOP_INPUT,
    TIMER_INPUT                      LCARD_AD.TIMER_INPUT,
    TIMER_INPUT_INTR                 LCARD_AD.TIMER_INPUT_INTR,
    RESERVED4                        LCARD_AD.RESERVED4,
    GET_TABLE                        LCARD_AD.GET_TABLE,
    CONFIG_LC227                     LCARD_AD.CONFIG_LC227,
    GET_SAMPLE_LC227                 LCARD_AD.GET_SAMPLE_LC227,
    STATUS_LC227                     LCARD_AD.STATUS_LC227,
    GET_KADR_LC227                   LCARD_AD.GET_KADR_LC227,
    LOAD_BIOS_LC227                  LCARD_AD.LOAD_BIOS_LC227,
    GET_ERROR_HANDLER                LCARD_AD.GET_ERROR_HANDLER,
    GET_TIMEOUT                      LCARD_AD.GET_TIMEOUT,
    PLATA_TEST_CC                    LCARD_AD.PLATA_TEST_CC,
    MEMORY_STATE_CC                  LCARD_AD.MEMORY_STATE_CC,
    MEMORY_PM_STATE_CC               LCARD_AD.MEMORY_PM_STATE_CC,
    EXECUTE_COMMAND_CC               LCARD_AD.EXECUTE_COMMAND_CC,
    SET_CALIBR_MODE_CC               LCARD_AD.SET_CALIBR_MODE_CC,
    SET_ERROR_HANDLER                LCARD_AD.SET_ERROR_HANDLER,
    OUTDA_LC301                      LCARD_AD.OUTDA_LC301,
    SAMPLE_LC301                     LCARD_AD.SAMPLE_LC301,
    SAMPLE_LC111                     LCARD_AD.SAMPLE_LC111,
    SET_FIFO_SIZE_CC                 LCARD_AD.SET_FIFO_SIZE_CC,
    CONFIG_FIFO_CC                   LCARD_AD.CONFIG_FIFO_CC,
    SOFT_CONFIG_CC                   LCARD_AD.SOFT_CONFIG_CC,
    SOFT_START_CC                    LCARD_AD.SOFT_START_CC,
    SOFT_STOP_CC                     LCARD_AD.SOFT_STOP_CC,
    GET_NWORDS_CC                    LCARD_AD.GET_NWORDS_CC,
    GET_SOFT_DATA_CC                 LCARD_AD.GET_SOFT_DATA_CC,
    SOFT_CC                          LCARD_AD.SOFT_CC,
    FAST_SOFT_IRQ_START_CC           LCARD_AD.FAST_SOFT_IRQ_START_CC,
    GET_FAST_SOFT_DATA               LCARD_AD.GET_FAST_SOFT_DATA,
    FAST_SOFT_START_CC               LCARD_AD.FAST_SOFT_START_CC,
    GET_FAST_SOFT_IRQ_DATA           LCARD_AD.GET_FAST_SOFT_IRQ_DATA,
    FAST_SOFT_IRQ_STOP_CC            LCARD_AD.FAST_SOFT_IRQ_STOP_CC,
    WAIT_SOFT_DATA_CC                LCARD_AD.WAIT_SOFT_DATA_CC,
    GET_CTRL_LC301                   LCARD_AD.GET_CTRL_LC301,
    SET_CTRL_LC301                   LCARD_AD.SET_CTRL_LC301,
    READ_REG_7710                    LCARD_AD.READ_REG_7710,
    WRITE_REG_7710                   LCARD_AD.WRITE_REG_7710,
    LOAD_BIOS_LC351                  LCARD_AD.LOAD_BIOS_LC351,
    MEMORY_STATE_LC351               LCARD_AD.MEMORY_STATE_LC351,
    SET_CTRL_LC351                   LCARD_AD.SET_CTRL_LC351,
    OUTDA_LC351                      LCARD_AD.OUTDA_LC351,
    LOAD_DATA_LC351                  LCARD_AD.LOAD_DATA_LC351,
    START_OUT_LC351                  LCARD_AD.START_OUT_LC351,
    LOAD_BIOS_LC451                  LCARD_AD.LOAD_BIOS_LC451,
    INP_DIGITS_401                   LCARD_AD.INP_DIGITS_401,
    ENABLE_IRQ_401                   LCARD_AD.ENABLE_IRQ_401,
    OUT_DIGITS_402                   LCARD_AD.OUT_DIGITS_402,
    ENABLE_IRQ_402                   LCARD_AD.ENABLE_IRQ_402,
    OUT_DIGITS_403                   LCARD_AD.OUT_DIGITS_403,
    INP_DIGITS_403                   LCARD_AD.INP_DIGITS_403,
    ENABLE_IRQ_403                   LCARD_AD.ENABLE_IRQ_403,
    ENABLE_OUT_403                   LCARD_AD.ENABLE_OUT_403,
    READ_IO_403                      LCARD_AD.READ_IO_403,
    RESET_ANSW_403                   LCARD_AD.RESET_ANSW_403,
    PROGRAM_FILTER_LC201             LCARD_AD.PROGRAM_FILTER_LC201,
    PROGRAM_USIL_LC201               LCARD_AD.PROGRAM_USIL_LC201,
    PROGRAM_FILTER_LC210             LCARD_AD.PROGRAM_FILTER_LC210,
    PROGRAM_USIL_LC210               LCARD_AD.PROGRAM_USIL_LC210,
    READ_FLASH_CC                    LCARD_AD.READ_FLASH_CC,
    WRITE_FLASH_CC                   LCARD_AD.WRITE_FLASH_CC,
    WRITE_EN_DS_CC                   LCARD_AD.WRITE_EN_DS_CC,
    PUT_REMOTE_WORD_CC               LCARD_AD.PUT_REMOTE_WORD_CC,
    GET_REMOTE_WORD_CC               LCARD_AD.GET_REMOTE_WORD_CC,
    PUT_REMOTE_ARRAY_CC              LCARD_AD.PUT_REMOTE_ARRAY_CC,
    GET_REMOTE_ARRAY_CC              LCARD_AD.GET_REMOTE_ARRAY_CC,
    SET_IRQ_MASK_CC                  LCARD_AD.SET_IRQ_MASK_CC,
    GET_MODULE_IRQ                   LCARD_AD.GET_MODULE_IRQ,
    SET_TIMEOUT                      LCARD_AD.SET_TIMEOUT,
    LOW_POWER_CC                     LCARD_AD.LOW_POWER_CC,
    OUTDA_LC302                      LCARD_AD.OUTDA_LC302,
    KADR_LC302                       LCARD_AD.KADR_LC302,
    SET_CTRL_LC302                   LCARD_AD.SET_CTRL_LC302,
    PROGRAM_AD8402                   LCARD_AD.PROGRAM_AD8402,
    PROGRAM_MAX                      LCARD_AD.PROGRAM_MAX,
    OUTDA_AD8842                     LCARD_AD.OUTDA_AD8842,
    RELEASEDMACHANNEL                LCARD_AD.RELEASEDMACHANNEL,
    FORCE_INTER_DELAY_CC             LCARD_AD.FORCE_INTER_DELAY_CC,
    CONNECT_LC501                    LCARD_AD.CONNECT_LC501,
    ADCHAN_L241                      LCARD_AD.ADCHAN_L241,
    SELFCALIBR_L241                  LCARD_AD.SELFCALIBR_L241,
    SET_INTERFACE_TYPE               LCARD_AD.SET_INTERFACE_TYPE,
    SET_DEVICE_BINDING               LCARD_AD.SET_DEVICE_BINDING,
    SET_CRAIT_ADDRESS                LCARD_AD.SET_CRAIT_ADDRESS,
    GET_INI_SETTINGS                 LCARD_AD.GET_INI_SETTINGS,
    CONFIG_LC451                     LCARD_AD.CONFIG_LC451,
    STATUS_LC451                     LCARD_AD.STATUS_LC451,
    GET_SAMPLE_LC451                 LCARD_AD.GET_SAMPLE_LC451,
    GET_KADR_LC451                   LCARD_AD.GET_KADR_LC451,
    SET_THRESHOLD_LC451              LCARD_AD.SET_THRESHOLD_LC451,
    SET_IRQ_INFOM_CC                 LCARD_AD.SET_IRQ_INFOM_CC,
    SET_LC227DATA_IRQSET_CC          LCARD_AD.SET_LC227DATA_IRQSET_CC,
    GET_IRQ1DATA_CC                  LCARD_AD.GET_IRQ1DATA_CC,
    GET_LC227CHMASK                  LCARD_AD.GET_LC227CHMASK,
    REQUESTDMACHANNEL                LCARD_AD.REQUESTDMACHANNEL,
    CALIBRLC201_STEP1_BEG            LCARD_AD.CALIBRLC201_STEP1_BEG,
    CALIBRLC201_STEP1_CYCLE          LCARD_AD.CALIBRLC201_STEP1_CYCLE,
    CALIBRLC201_STEP1_FIN            LCARD_AD.CALIBRLC201_STEP1_FIN,
    CALIBRLC201_STEP2_BEG            LCARD_AD.CALIBRLC201_STEP2_BEG,
    CALIBRLC201_STEP2_CYCLE_CHANV0   LCARD_AD.CALIBRLC201_STEP2_CYCLE_CHANV0,
    CALIBRLC201_STEP2_CYCLE_CHANV5   LCARD_AD.CALIBRLC201_STEP2_CYCLE_CHANV5,
    CALIBRLC201_STEP2_CYCLE_CHANZG   LCARD_AD.CALIBRLC201_STEP2_CYCLE_CHANZG,
    CALIBRLC201_STEP2_CYCLE_GAIN     LCARD_AD.CALIBRLC201_STEP2_CYCLE_GAIN,
    CALIBRLC201_STEP2_FIN            LCARD_AD.CALIBRLC201_STEP2_FIN,
    CALIBR_LC201_STEP1               LCARD_AD.CALIBR_LC201_STEP1,
    CALIBR_LC201_STEP2               LCARD_AD.CALIBR_LC201_STEP2,
    GET_DFLTCALIBRSET_LC201          LCARD_AD.GET_DFLTCALIBRSET_LC201,
    SETU_LC301                       LCARD_AD.SETU_LC301,
    SET_DFLTCALIBRSET_LC201          LCARD_AD.SET_DFLTCALIBRSET_LC201,
    SET_TRIM_DAC_LC201_FILE          LCARD_AD.SET_TRIM_DAC_LC201_FILE,
    READ_REG_7710_CRAIT              LCARD_AD.READ_REG_7710_CRAIT,
    WRITE_REG_7710_CRAIT             LCARD_AD.WRITE_REG_7710_CRAIT,
    CHECK_OVERFLOW_7710_CRAIT        LCARD_AD.CHECK_OVERFLOW_7710_CRAIT,
    ENABLE_7710_CRAIT                LCARD_AD.ENABLE_7710_CRAIT,
    FINISH_READ_7710_CRAIT           LCARD_AD.FINISH_READ_7710_CRAIT,
    FINISH_READ_CODE_7710_CRAIT      LCARD_AD.FINISH_READ_CODE_7710_CRAIT,
    IS_7710_PRESENT_CRAIT            LCARD_AD.IS_7710_PRESENT_CRAIT,
    IS_7710_READY_CRAIT              LCARD_AD.IS_7710_READY_CRAIT,
    READ_7710_CRAIT                  LCARD_AD.READ_7710_CRAIT,
    READ_CODE_7710_CRAIT             LCARD_AD.READ_CODE_7710_CRAIT,
    RESET_FILTER_7710_CRAIT          LCARD_AD.RESET_FILTER_7710_CRAIT,
    SELF_CALIBR_7710_CRAIT           LCARD_AD.SELF_CALIBR_7710_CRAIT,
    SET_CHANNEL_7710_CRAIT           LCARD_AD.SET_CHANNEL_7710_CRAIT,
    CREATE_CHANNEL_LC201             LCARD_AD.CREATE_CHANNEL_LC201,
    KADR_LC227                       LCARD_AD.KADR_LC227,
    SET_CALIBRATION_LC227            LCARD_AD.SET_CALIBRATION_LC227,
    SET_CALIBRATION_LC227_ALL        LCARD_AD.SET_CALIBRATION_LC227_ALL,
    GET_LC201_CONNECTDAC_MODE        LCARD_AD.GET_LC201_CONNECTDAC_MODE,
    SET_LC201_CONNECTDAC_MODE        LCARD_AD.SET_LC201_CONNECTDAC_MODE,
    INIT_LC201_FROM_FILE             LCARD_AD.INIT_LC201_FROM_FILE,
    INIT_LC201_FROM_PPZU             LCARD_AD.INIT_LC201_FROM_PPZU,
    KADR_LC451                       LCARD_AD.KADR_LC451,
    INIT_MODULE_LC201                LCARD_AD.INIT_MODULE_LC201,
    TRANSMIT_CALIBR_DATA201_TO_PPZU  LCARD_AD.TRANSMIT_CALIBR_DATA201_TO_PPZU,
    IN_BYTE                          LCARD_AD.IN_BYTE,
    IN_WORD                          LCARD_AD.IN_WORD,
    OUT_BYTE                         LCARD_AD.OUT_BYTE,
    OUT_WORD                         LCARD_AD.OUT_WORD,
    RESET_SYNMODE                    LCARD_AD.RESET_SYNMODE,
    SET_SYNMODE_ADC                  LCARD_AD.SET_SYNMODE_ADC,
    SET_SYNMODE_TTL                  LCARD_AD.SET_SYNMODE_TTL,
    START_SYNSOFT                    LCARD_AD.START_SYNSOFT,
    SYNSOFT_CC                       LCARD_AD.SYNSOFT_CC,
    LOADBIOS_MODULE_CC               LCARD_AD.LOADBIOS_MODULE_CC,
    CREATE_CHANNEL_LC101             LCARD_AD.CREATE_CHANNEL_LC101,
    CREATE_CHANNEL_LC102             LCARD_AD.CREATE_CHANNEL_LC102,
    CREATE_CHANNEL_LC104             LCARD_AD.CREATE_CHANNEL_LC104,
    CREATE_CHANNEL_LC111             LCARD_AD.CREATE_CHANNEL_LC111,
    CREATE_CHANNEL_LC210             LCARD_AD.CREATE_CHANNEL_LC210,
    DEINSTALLLOGIO                   LCARD_AD.DEINSTALLLOGIO,
    INSTALLLOGIO                     LCARD_AD.INSTALLLOGIO,
    CREATE_CONTROL_WORD_LC302        LCARD_AD.CREATE_CONTROL_WORD_LC302,
    CREATE_FAST_CHAN_CC              LCARD_AD.CREATE_FAST_CHAN_CC,
    KADR_OUT_LC302_FAST_CC           LCARD_AD.KADR_OUT_LC302_FAST_CC,
    OUT_LC302_FAST_CC                LCARD_AD.OUT_LC302_FAST_CC,
    READ_FAST_KADR_CC                LCARD_AD.READ_FAST_KADR_CC,
    READ_FAST_SAMPLE_CC              LCARD_AD.READ_FAST_SAMPLE_CC,
    LOADCRAIT                        LCARD_AD.LOADCRAIT,
    AUTO_PREPARE_MODULE              LCARD_AD.AUTO_PREPARE_MODULE,
    _GET_DATA                        LCARD_AD._GET_DATA,
    _PUT_DATA                        LCARD_AD._PUT_DATA,
    _SEND_COMMAND                    LCARD_AD._SEND_COMMAND,
    FAST_LOADING_LC010               LCARD_AD.FAST_LOADING_LC010,
    FAST_LOADING_LCI01               LCARD_AD.FAST_LOADING_LCI01
