ALIAS
    '_SELECT_SLOT@4'                     =SELECT_SLOT,
    '_PLATA_TEST@0'                      =PLATA_TEST,
    '_SET_BOARD_TYPE@4'                  =SET_BOARD_TYPE,
    '_GET_BOARD_TYPE@0'                  =GET_BOARD_TYPE,
    '_SET_BASE_ADDRESS@4'                =SET_BASE_ADDRESS,
    '_ENABLE_INT@4'                      =ENABLE_INT,
    '_CREATE_CHANNEL@12'                 =CREATE_CHANNEL,
    '_MEMORY_STATE@0'                    =MEMORY_STATE,
    '_MEMORY_PM_STATE@0'                 =MEMORY_PM_STATE,
    '_SET_INTER_DELAY@4'                 =SET_INTER_DELAY,
    '_SET_ADSP_SPEED@4'                  =SET_ADSP_SPEED,
    '_SET_WAIT_STATE@4'                  =SET_WAIT_STATE,
    '_SET_TIMER_SCALE@4'                 =SET_TIMER_SCALE,
    '_TIMER_L154_L164@12'                =TIMER_L154_L164,
    '_WAIT_TICK_L154_L164@4'             =WAIT_TICK_L154_L164,
    '_GET_TIMER_L154_L164@0'             =GET_TIMER_L154_L164,
    '_CALIBRATION@0'                     =CALIBRATION,
    '_INIT_COMPARATOR@16'                =INIT_COMPARATOR,
    '_LOW_POWER@4'                       =LOW_POWER,
    '_GET_SLOT_CODE@8'                   =GET_SLOT_CODE,
    '_RESET_ALL@0'                       =RESET_ALL,
    '_MAKE_CHANNEL@20'                   =MAKE_CHANNEL,
    '_PROGRAM_FILTER@16'                 =PROGRAM_FILTER,
    '_PROGRAM_LM_201@20'                 =PROGRAM_LM_201,
    '_PROGRAM_LM_102@12'                 =PROGRAM_LM_102,
    '_PROGRAM_LM_501@36'                 =PROGRAM_LM_501,
    '_PROGRAM_LM_DAC@20'                 =PROGRAM_LM_DAC,
    '_GET_LM_401@8'                      =GET_LM_401,
    '_LM_404@4'                          =LM_404,
    '_PROGRAM_LM_TTLOUT@12'              =PROGRAM_LM_TTLOUT,
    '_SETCHANNEL@4'                      =SETCHANNEL,
    '_SAMPLE@0'                          =SAMPLE,
    '_ADCHAN@4'                          =ADCHAN,
    '_KADR@12'                           =KADR,
    '_STREAM@16'                         =STREAM,
    '_SOFT@20'                           =SOFT,
    '_SOFT_HUGE@20'                      =SOFT_HUGE,
    '_DMAONE@20'                         =DMAONE,
    '_DMAALL@24'                         =DMAALL,
    '_DMA_ALL_DA@40'                     =DMA_ALL_DA,
    '_OUTDA@4'                           =OUTDA,
    '_SET_DA_NUMBER@8'                   =SET_DA_NUMBER,
    '_STREAM_OUTDA@4'                    =STREAM_OUTDA,
    '_DASTREAM@12'                       =DASTREAM,
    '_DASTREAM_HUGE@12'                  =DASTREAM_HUGE,
    '_DADMASTREAM@16'                    =DADMASTREAM,
    '_OUTBYTE@4'                         =OUTBYTE,
    '_INPBYTE@0'                         =INPBYTE,
    '_DSP_INPBYTE@0'                     =DSP_INPBYTE,
    '_DSP_OUTBYTE@4'                     =DSP_OUTBYTE,
    '_INTR_SETUP@4'                      =INTR_SETUP,
    '_STOP_INTR@0'                       =STOP_INTR,
    '_RESET_IRQ@0'                       =RESET_IRQ,
    '_INIT_SIMPLE_INTR@12'               =INIT_SIMPLE_INTR,
    '_STREAM_INTR@12'                    =STREAM_INTR,
    '_SOFT_INTR@16'                      =SOFT_INTR,
    '_READ_DATA@0'                       =READ_DATA,
    '_DATA_READY@0'                      =DATA_READY,
    '_SYNCHRO_MODE@16'                   =SYNCHRO_MODE,
    '_SOFT_MEMORY_START@28'              =SOFT_MEMORY_START,
    '_TEST_FOR_INPUT_END@0'              =TEST_FOR_INPUT_END,
    '_GET_INPUT_DATA@8'                  =GET_INPUT_DATA,
    '_SOFT_MEMORY_RESTART@0'             =SOFT_MEMORY_RESTART,
    '_DMA_OFF@0'                         =DMA_OFF,
    '_DMA_TEST@0'                        =DMA_TEST,
    '_DMA_COUNTER_IN@0'                  =DMA_COUNTER_IN,
    '_DMA_COUNTER_OUT@0'                 =DMA_COUNTER_OUT,
    '_GET_BUFFER@4'                      =GET_BUFFER,
    '_GET_BUFFER_HALF@4'                 =GET_BUFFER_HALF,
    '_PUT_BUFFER@4'                      =PUT_BUFFER,
    '_PUT_BUFFER_HALF@4'                 =PUT_BUFFER_HALF,
    '_CONFIG_FIFO@4'                     =CONFIG_FIFO,
    '_CONFIG_2FIFO_TYPE@8'               =CONFIG_2FIFO_TYPE,
    '_READ_FIFO@8'                       =READ_FIFO,
    '_STREAM_FIFO2_BEGIN@16'             =STREAM_FIFO2_BEGIN,
    '_GET_DIGITS_1056@8'                 =GET_DIGITS_1056,
    '_OUT_DIGITS_1056@4'                 =OUT_DIGITS_1056,
    '_STREAM_1056@16'                    =STREAM_1056,
    '_STREAM_DMA_1056@20'                =STREAM_DMA_1056,
    '_OUT_STREAM_1056@12'                =OUT_STREAM_1056,
    '_OUT_STREAM_DMA_1056@16'            =OUT_STREAM_DMA_1056,
    '_INIT_INTR_1056@12'                 =INIT_INTR_1056,
    '_SET_SYNCHRO_MODE_1056@12'          =SET_SYNCHRO_MODE_1056,
    '_ZERO_MODE_1208@4'                  =ZERO_MODE_1208,
    '_OUTDA_1208@8'                      =OUTDA_1208,
    '_KADR_1208@12'                      =KADR_1208,
    '_SOFT_1208@20'                      =SOFT_1208,
    '_SOFT_FON_1208@20'                  =SOFT_FON_1208,
    '_DMASOFT_1208@24'                   =DMASOFT_1208,
    '_SOFT_INTR_1208@12'                 =SOFT_INTR_1208,
    '_GET_DATA@0'                        =GET_DATA,
    '_PUT_DATA@4'                        =PUT_DATA,
    '_READ_INT_MEMORY@16'                =READ_INT_MEMORY,
    '_WRITE_INT_MEMORY@16'               =WRITE_INT_MEMORY,
    '_LOADBIOS@8'                        =LOADBIOS,
    '_POWER_AND_PRINTER_E330@8'          =POWER_AND_PRINTER_E330,
    '_SET_EPP_MODE_E330@4'               =SET_EPP_MODE_E330,
    '_SET_FIFO_PARAMETERS_E330@8'        =SET_FIFO_PARAMETERS_E330,
    '_SET_SOFT_PARM_E330@8'              =SET_SOFT_PARM_E330,
    '_SET_TIME_PARAMETERS_E330@4'        =SET_TIME_PARAMETERS_E330,
    '_TIMER_INPUT_START_E330@0'          =TIMER_INPUT_START_E330,
    '_STOP_FUNC_E330@0'                  =STOP_FUNC_E330,
    '_TIMER_INPUT_E330@8'                =TIMER_INPUT_E330,
    '_SOFT_MEMORY_PREPARE_E330@16'       =SOFT_MEMORY_PREPARE_E330,
    '_SOFT_MEMORY_START_E330@0'          =SOFT_MEMORY_START_E330,
    '_TIMER_INPUT_IRQ_START_E330@4'      =TIMER_INPUT_IRQ_START_E330,
    '_IRQ_SLOW_START_E330@8'             =IRQ_SLOW_START_E330,
    '_SET_TEST_SPEED_MODE_E330@4'        =SET_TEST_SPEED_MODE_E330,
    '_WRITE_BY_ADDRESS_E330@8'           =WRITE_BY_ADDRESS_E330,
    '_READ_BY_ADDRESS_E330@4'            =READ_BY_ADDRESS_E330,
    '_BOARD_SPECIFIC_INIT@4'             =BOARD_SPECIFIC_INIT,
    '_SELECT_BOARD@4'                    =SELECT_BOARD,
    '_SETBASEADDRESS@4'                  =SETBASEADDRESS,
    '_EXEC_ADSP_COMMAND@20'              =EXEC_ADSP_COMMAND,
    '_GET_STATUS@0'                      =GET_STATUS,
    '_ALLOCATEBUFFER@12'                 =ALLOCATEBUFFER,
    '_CONFIG_TX_CHANNEL_LCI01@4'         =CONFIG_TX_CHANNEL_LCI01,
    '_FREEBUFFER@4'                      =FREEBUFFER,
    '_GET_HALF_FIFO@12'                  =GET_HALF_FIFO,
    '_GET_INPUT_POINTS@4'                =GET_INPUT_POINTS,
    '_QADCHAN@4'                         =QADCHAN,
    '_LOADBIOSFROMARRAY_L1211@4'         =LOADBIOSFROMARRAY_L1211,
    '_INIT_CORRECTION_LC302@4'           =INIT_CORRECTION_LC302,
    '_QSOFT@8'                           =QSOFT,
    '_RESERVED2@12'                      =RESERVED2,
    '_READ_CALIBR_CC@0'                  =READ_CALIBR_CC,
    '_CONFIG_RX_CHANNEL_LCI01@4'         =CONFIG_RX_CHANNEL_LCI01,
    '_SELECT_DEVICE@4'                   =SELECT_DEVICE,
    '_SET_AD_MODE@4'                     =SET_AD_MODE,
    '_CONFIGURE_FAST_READ_CC@8'          =CONFIGURE_FAST_READ_CC,
    '_SET_CHANNELS@8'                    =SET_CHANNELS,
    '_INITIALIZE_CORRECTION_PC@4'        =INITIALIZE_CORRECTION_PC,
    '_SET_DAC_BUFER_E330@8'              =SET_DAC_BUFER_E330,
    '_SET_TIME@12'                       =SET_TIME,
    '_SET_FAST_PARAMS_CC@12'             =SET_FAST_PARAMS_CC,
    '_START_LOOP_DAC_E330@0'             =START_LOOP_DAC_E330,
    '_STOP_INPUT@0'                      =STOP_INPUT,
    '_TIMER_INPUT@0'                     =TIMER_INPUT,
    '_TIMER_INPUT_INTR@4'                =TIMER_INPUT_INTR,
    '_RESERVED4@12'                      =RESERVED4,
    '_GET_TABLE@8'                       =GET_TABLE,
    '_CONFIG_LC227@12'                   =CONFIG_LC227,
    '_GET_SAMPLE_LC227@12'               =GET_SAMPLE_LC227,
    '_STATUS_LC227@4'                    =STATUS_LC227,
    '_GET_KADR_LC227@16'                 =GET_KADR_LC227,
    '_LOAD_BIOS_LC227@8'                 =LOAD_BIOS_LC227,
    '_GET_ERROR_HANDLER@0'               =GET_ERROR_HANDLER,
    '_GET_TIMEOUT@0'                     =GET_TIMEOUT,
    '_PLATA_TEST_CC@0'                   =PLATA_TEST_CC,
    '_MEMORY_STATE_CC@0'                 =MEMORY_STATE_CC,
    '_MEMORY_PM_STATE_CC@0'              =MEMORY_PM_STATE_CC,
    '_EXECUTE_COMMAND_CC@20'             =EXECUTE_COMMAND_CC,
    '_SET_CALIBR_MODE_CC@4'              =SET_CALIBR_MODE_CC,
    '_SET_ERROR_HANDLER@4'               =SET_ERROR_HANDLER,
    '_OUTDA_LC301@12'                    =OUTDA_LC301,
    '_SAMPLE_LC301@12'                   =SAMPLE_LC301,
    '_SAMPLE_LC111@8'                    =SAMPLE_LC111,
    '_SET_FIFO_SIZE_CC@4'                =SET_FIFO_SIZE_CC,
    '_CONFIG_FIFO_CC@8'                  =CONFIG_FIFO_CC,
    '_SOFT_CONFIG_CC@16'                 =SOFT_CONFIG_CC,
    '_SOFT_START_CC@0'                   =SOFT_START_CC,
    '_SOFT_STOP_CC@0'                    =SOFT_STOP_CC,
    '_GET_NWORDS_CC@4'                   =GET_NWORDS_CC,
    '_GET_SOFT_DATA_CC@8'                =GET_SOFT_DATA_CC,
    '_SOFT_CC@24'                        =SOFT_CC,
    '_FAST_SOFT_IRQ_START_CC@4'          =FAST_SOFT_IRQ_START_CC,
    '_GET_FAST_SOFT_DATA@8'              =GET_FAST_SOFT_DATA,
    '_FAST_SOFT_START_CC@0'              =FAST_SOFT_START_CC,
    '_GET_FAST_SOFT_IRQ_DATA@8'          =GET_FAST_SOFT_IRQ_DATA,
    '_FAST_SOFT_IRQ_STOP_CC@0'           =FAST_SOFT_IRQ_STOP_CC,
    '_WAIT_SOFT_DATA_CC@8'               =WAIT_SOFT_DATA_CC,
    '_GET_CTRL_LC301@4'                  =GET_CTRL_LC301,
    '_SET_CTRL_LC301@8'                  =SET_CTRL_LC301,
    '_READ_REG_7710@12'                  =READ_REG_7710,
    '_WRITE_REG_7710@12'                 =WRITE_REG_7710,
    '_LOAD_BIOS_LC351@8'                 =LOAD_BIOS_LC351,
    '_MEMORY_STATE_LC351@4'              =MEMORY_STATE_LC351,
    '_SET_CTRL_LC351@12'                 =SET_CTRL_LC351,
    '_OUTDA_LC351@8'                     =OUTDA_LC351,
    '_LOAD_DATA_LC351@16'                =LOAD_DATA_LC351,
    '_START_OUT_LC351@12'                =START_OUT_LC351,
    '_LOAD_BIOS_LC451@8'                 =LOAD_BIOS_LC451,
    '_INP_DIGITS_401@4'                  =INP_DIGITS_401,
    '_ENABLE_IRQ_401@8'                  =ENABLE_IRQ_401,
    '_OUT_DIGITS_402@8'                  =OUT_DIGITS_402,
    '_ENABLE_IRQ_402@8'                  =ENABLE_IRQ_402,
    '_OUT_DIGITS_403@8'                  =OUT_DIGITS_403,
    '_INP_DIGITS_403@4'                  =INP_DIGITS_403,
    '_ENABLE_IRQ_403@8'                  =ENABLE_IRQ_403,
    '_ENABLE_OUT_403@8'                  =ENABLE_OUT_403,
    '_READ_IO_403@4'                     =READ_IO_403,
    '_RESET_ANSW_403@4'                  =RESET_ANSW_403,
    '_PROGRAM_FILTER_LC201@8'            =PROGRAM_FILTER_LC201,
    '_PROGRAM_USIL_LC201@12'             =PROGRAM_USIL_LC201,
    '_PROGRAM_FILTER_LC210@8'            =PROGRAM_FILTER_LC210,
    '_PROGRAM_USIL_LC210@12'             =PROGRAM_USIL_LC210,
    '_READ_FLASH_CC@8'                   =READ_FLASH_CC,
    '_WRITE_FLASH_CC@12'                 =WRITE_FLASH_CC,
    '_WRITE_EN_DS_CC@8'                  =WRITE_EN_DS_CC,
    '_PUT_REMOTE_WORD_CC@8'              =PUT_REMOTE_WORD_CC,
    '_GET_REMOTE_WORD_CC@4'              =GET_REMOTE_WORD_CC,
    '_PUT_REMOTE_ARRAY_CC@16'            =PUT_REMOTE_ARRAY_CC,
    '_GET_REMOTE_ARRAY_CC@16'            =GET_REMOTE_ARRAY_CC,
    '_SET_IRQ_MASK_CC@4'                 =SET_IRQ_MASK_CC,
    '_GET_MODULE_IRQ@8'                  =GET_MODULE_IRQ,
    '_SET_TIMEOUT@4'                     =SET_TIMEOUT,
    '_LOW_POWER_CC@4'                    =LOW_POWER_CC,
    '_OUTDA_LC302@12'                    =OUTDA_LC302,
    '_KADR_LC302@12'                     =KADR_LC302,
    '_SET_CTRL_LC302@8'                  =SET_CTRL_LC302,
    '_PROGRAM_AD8402@16'                 =PROGRAM_AD8402,
    '_PROGRAM_MAX@12'                    =PROGRAM_MAX,
    '_OUTDA_AD8842@12'                   =OUTDA_AD8842,
    '_RELEASEDMACHANNEL@4'               =RELEASEDMACHANNEL,
    '_FORCE_INTER_DELAY_CC@4'            =FORCE_INTER_DELAY_CC,
    '_CONNECT_LC501@8'                   =CONNECT_LC501,
    '_ADCHAN_L241@4'                     =ADCHAN_L241,
    '_SELFCALIBR_L241@8'                 =SELFCALIBR_L241,
    '_SET_INTERFACE_TYPE@4'              =SET_INTERFACE_TYPE,
    '_SET_DEVICE_BINDING@4'              =SET_DEVICE_BINDING,
    '_SET_CRAIT_ADDRESS@4'               =SET_CRAIT_ADDRESS,
    '_GET_INI_SETTINGS@0'                =GET_INI_SETTINGS,
    '_CONFIG_LC451@12'                   =CONFIG_LC451,
    '_STATUS_LC451@4'                    =STATUS_LC451,
    '_GET_SAMPLE_LC451@12'               =GET_SAMPLE_LC451,
    '_GET_KADR_LC451@16'                 =GET_KADR_LC451,
    '_SET_THRESHOLD_LC451@16'            =SET_THRESHOLD_LC451,
    '_SET_IRQ_INFOM_CC@8'                =SET_IRQ_INFOM_CC,
    '_SET_LC227DATA_IRQSET_CC@0'         =SET_LC227DATA_IRQSET_CC,
    '_GET_IRQ1DATA_CC@12'                =GET_IRQ1DATA_CC,
    '_GET_LC227CHMASK@8'                 =GET_LC227CHMASK,
    '_REQUESTDMACHANNEL@16'              =REQUESTDMACHANNEL,
    '_CALIBRLC201_STEP1_BEG@8'           =CALIBRLC201_STEP1_BEG,
    '_CALIBRLC201_STEP1_CYCLE@12'        =CALIBRLC201_STEP1_CYCLE,
    '_CALIBRLC201_STEP1_FIN@4'           =CALIBRLC201_STEP1_FIN,
    '_CALIBRLC201_STEP2_BEG@8'           =CALIBRLC201_STEP2_BEG,
    '_CALIBRLC201_STEP2_CYCLE_CHANV0@12' =CALIBRLC201_STEP2_CYCLE_CHANV0,
    '_CALIBRLC201_STEP2_CYCLE_CHANV5@12' =CALIBRLC201_STEP2_CYCLE_CHANV5,
    '_CALIBRLC201_STEP2_CYCLE_CHANZG@16' =CALIBRLC201_STEP2_CYCLE_CHANZG,
    '_CALIBRLC201_STEP2_CYCLE_GAIN@8'    =CALIBRLC201_STEP2_CYCLE_GAIN,
    '_CALIBRLC201_STEP2_FIN@4'           =CALIBRLC201_STEP2_FIN,
    '_CALIBR_LC201_STEP1@8'              =CALIBR_LC201_STEP1,
    '_CALIBR_LC201_STEP2@8'              =CALIBR_LC201_STEP2,
    '_GET_DFLTCALIBRSET_LC201@28'        =GET_DFLTCALIBRSET_LC201,
    '_SETU_LC301@12'                     =SETU_LC301,
    '_SET_DFLTCALIBRSET_LC201@28'        =SET_DFLTCALIBRSET_LC201,
    '_SET_TRIM_DAC_LC201_FILE@16'        =SET_TRIM_DAC_LC201_FILE,
    '_READ_REG_7710_CRAIT@12'            =READ_REG_7710_CRAIT,
    '_WRITE_REG_7710_CRAIT@12'           =WRITE_REG_7710_CRAIT,
    '_CHECK_OVERFLOW_7710_CRAIT@0'       =CHECK_OVERFLOW_7710_CRAIT,
    '_ENABLE_7710_CRAIT@8'               =ENABLE_7710_CRAIT,
    '_FINISH_READ_7710_CRAIT@4'          =FINISH_READ_7710_CRAIT,
    '_FINISH_READ_CODE_7710_CRAIT@4'     =FINISH_READ_CODE_7710_CRAIT,
    '_IS_7710_PRESENT_CRAIT@4'           =IS_7710_PRESENT_CRAIT,
    '_IS_7710_READY_CRAIT@4'             =IS_7710_READY_CRAIT,
    '_READ_7710_CRAIT@4'                 =READ_7710_CRAIT,
    '_READ_CODE_7710_CRAIT@4'            =READ_CODE_7710_CRAIT,
    '_RESET_FILTER_7710_CRAIT@0'         =RESET_FILTER_7710_CRAIT,
    '_SELF_CALIBR_7710_CRAIT@8'          =SELF_CALIBR_7710_CRAIT,
    '_SET_CHANNEL_7710_CRAIT@8'          =SET_CHANNEL_7710_CRAIT,
    '_CREATE_CHANNEL_LC201@16'           =CREATE_CHANNEL_LC201,
    '_KADR_LC227@16'                     =KADR_LC227,
    '_SET_CALIBRATION_LC227@4'           =SET_CALIBRATION_LC227,
    '_SET_CALIBRATION_LC227_ALL@0'       =SET_CALIBRATION_LC227_ALL,
    '_GET_LC201_CONNECTDAC_MODE@0'       =GET_LC201_CONNECTDAC_MODE,
    '_SET_LC201_CONNECTDAC_MODE@4'       =SET_LC201_CONNECTDAC_MODE,
    '_INIT_LC201_FROM_FILE@32'           =INIT_LC201_FROM_FILE,
    '_INIT_LC201_FROM_PPZU@24'           =INIT_LC201_FROM_PPZU,
    '_KADR_LC451@20'                     =KADR_LC451,
    '_INIT_MODULE_LC201@28'              =INIT_MODULE_LC201,
    '_TRANSMIT_CALIBR_DATA201_TO_PPZU@12'=TRANSMIT_CALIBR_DATA201_TO_PPZU,
    '_IN_BYTE@4'                         =IN_BYTE,
    '_IN_WORD@4'                         =IN_WORD,
    '_OUT_BYTE@8'                        =OUT_BYTE,
    '_OUT_WORD@8'                        =OUT_WORD,
    '_RESET_SYNMODE@0'                   =RESET_SYNMODE,
    '_SET_SYNMODE_ADC@20'                =SET_SYNMODE_ADC,
    '_SET_SYNMODE_TTL@16'                =SET_SYNMODE_TTL,
    '_START_SYNSOFT@0'                   =START_SYNSOFT,
    '_SYNSOFT_CC@24'                     =SYNSOFT_CC,
    '_LOADBIOS_MODULE_CC@12'             =LOADBIOS_MODULE_CC,
    '_CREATE_CHANNEL_LC101@12'           =CREATE_CHANNEL_LC101,
    '_CREATE_CHANNEL_LC102@12'           =CREATE_CHANNEL_LC102,
    '_CREATE_CHANNEL_LC104@12'           =CREATE_CHANNEL_LC104,
    '_CREATE_CHANNEL_LC111@12'           =CREATE_CHANNEL_LC111,
    '_CREATE_CHANNEL_LC210@12'           =CREATE_CHANNEL_LC210,
    '_DEINSTALLLOGIO@0'                  =DEINSTALLLOGIO,
    '_INSTALLLOGIO@0'                    =INSTALLLOGIO,
    '_CREATE_CONTROL_WORD_LC302@12'      =CREATE_CONTROL_WORD_LC302,
    '_CREATE_FAST_CHAN_CC@12'            =CREATE_FAST_CHAN_CC,
    '_KADR_OUT_LC302_FAST_CC@12'         =KADR_OUT_LC302_FAST_CC,
    '_OUT_LC302_FAST_CC@8'               =OUT_LC302_FAST_CC,
    '_READ_FAST_KADR_CC@8'               =READ_FAST_KADR_CC,
    '_READ_FAST_SAMPLE_CC@4'             =READ_FAST_SAMPLE_CC,
    '_LOADCRAIT@8'                       =LOADCRAIT,
    '_AUTO_PREPARE_MODULE@4'             =AUTO_PREPARE_MODULE,
    '__GET_DATA@0'                       =_GET_DATA,
    '__PUT_DATA@4'                       =_PUT_DATA,
    '__SEND_COMMAND@4'                   =_SEND_COMMAND,
    '_FAST_LOADING_LC010@4'              =FAST_LOADING_LC010,
    '_FAST_LOADING_LCI01@4'              =FAST_LOADING_LCI01
